{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Damhusåen"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Damhusåen","index":0,"n_rows":28,"n_cols":77,"rows_kept":28,"cut":false,"hidden":false,"merged":[[19,0,21,0],[19,59,21,59],[22,0,24,0],[22,59,24,59],[25,0,27,0],[25,59,27,59],[10,0,12,0],[10,59,12,59],[13,0,15,0],[13,59,15,59],[16,0,18,0],[16,59,18,59],[3,0,3,1],[3,59,3,60],[4,0,6,0],[4,59,6,59],[7,0,9,0],[7,59,9,59],[0,0,1,1],[0,2,1,4],[0,59,1,60],[0,61,1,63],[2,0,2,1],[2,59,2,60]]}
["Vandområde",null,"Damhusåen",{"$nulls":56},"Vandområde",null,"Damhusåen"]
[]
["Udlednings nr. ",null,"UD10b","UD10d","UD11b","UD12","UD13","UD14","UD15","UD16","UD17","UD18","UD19b","UD20b","UD21","UD21b","UD24",{"$nulls":42},"Udlednings nr. ",null,"UD10b","UD10d","UD11b","UD12","UD13","UD14","UD15","UD16","UD17","UD18","UD19b","UD20b","UD21","UD21b","UD24","Sum"]
["Adresse",null,"Nødoverløb Damhusåens renseanlæg","Hovedoverløb Damhus-ledning","Åhaven","Sønderkær","Vigerslev Allé","Gårdstedet","Heldbovej","Lykkebovej","Landlystvej","Skyttegårdsvej","Sandhusvej","Hvidovre station","Vigerslev-parken N for Dæmningen","Nødoverløb Torpedo-bygværket","Roskildevej","SUM",{"$nulls":41},"Adresse",null,"Nødoverløb Damhusåens renseanlæg","Hovedoverløb Damhus-ledning","Åhaven","Sønderkær","Vigerslev Allé","Gårdstedet","Heldbovej","Lykkebovej","Landlystvej","Skyttegårdsvej","Sandhusvej","Hvidovre station","Vigerslev-parken N for Dæmningen","Nødoverløb ved Torpedo-bygværket","Roskildevej","-"]
["Kloakeringstype","Status","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","-",{"$nulls":41},"Kloakeringstype","Status","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","-"]
[null,"Plan","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","-",{"$nulls":42},"Plan","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","-"]
[null,"Strategi","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","-",{"$nulls":42},"Strategi","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","-"]
["Reduceret areal       ha","Status",62.096269999999997,0,4.9262990000000002,13.292068,9.0631889999999995,1.4540759999999999,1.5233950000000001,3.503314,1.9389799999999999,4.8509120000000001,2.2999999999999998,1.07056,284.5,0,0,{"$f":"SUM(Tabel15[[#This Row],[Nødoverløb Damhusåens renseanlæg]:[Roskildevej]])","v":390.51906299999996},{"$nulls":41},"Reduceret areal       ha","Status",62.096269999999997,0,4.9262990000000002,13.292068,9.0631889999999995,1.4540759999999999,1.5233950000000001,3.503314,1.9389799999999999,4.8509120000000001,2.2999999999999998,1.07056,284.5,0,0,{"$f":"SUM(BJ8:BX8)","v":390.51906299999996}]
[null,"Plan",62.096269999999997,0,4.9262990000000002,13.292068,9.0631889999999995,1.4540759999999999,1.5233950000000001,3.503314,1.9389799999999999,4.8509120000000001,2.2999999999999998,1.07056,284.5,0,0,{"$f":"SUM(Tabel15[[#This Row],[Nødoverløb Damhusåens renseanlæg]:[Roskildevej]])","v":390.51906299999996},{"$nulls":42},"Plan",62.096269999999997,0,4.9262990000000002,13.292068,9.0631889999999995,1.4540759999999999,1.5233950000000001,3.503314,1.9389799999999999,4.8509120000000001,2.2999999999999998,1.07056,284.5,0,0,390.51906299999996]
[null,"Strategi",62.096269999999997,0,4.9262990000000002,13.292068,9.0631889999999995,1.4540759999999999,1.5233950000000001,3.503314,1.9389799999999999,4.8509120000000001,2.2999999999999998,1.07056,284.5,0,0,{"$f":"SUM(Tabel15[[#This Row],[Nødoverløb Damhusåens renseanlæg]:[Roskildevej]])","v":390.51906299999996},{"$nulls":42},"Strategi",62.096269999999997,0,4.9262990000000002,13.292068,9.0631889999999995,1.4540759999999999,1.5233950000000001,3.503314,1.9389799999999999,4.8509120000000001,2.2999999999999998,1.07056,284.5,0,0,390.51906299999996]
["Maks udledning        l/s","Status",5000,5000,700,3000,1200,500,100,300,300,500,500,200,1500,0,1000,{"$f":"SUM(Tabel15[[#This Row],[Nødoverløb Damhusåens renseanlæg]:[Roskildevej]])","v":19800},{"$nulls":41},"Maks udledning        l/s","Status",5000,5000,700,3000,1200,500,100,300,300,500,500,200,1500,0,1000,19800]
[null,"Plan",5000,5000,700,3000,1200,500,100,300,300,500,500,200,1500,0,1000,{"$f":"SUM(Tabel15[[#This Row],[Nødoverløb Damhusåens renseanlæg]:[Roskildevej]])","v":19800},{"$nulls":42},"Plan",5000,5000,700,3000,1200,500,100,300,300,500,500,200,1500,0,1000,19800]
[null,"Strategi",5000,5000,700,3000,1200,500,100,300,300,500,500,200,1500,0,1000,{"$f":"SUM(Tabel15[[#This Row],[Nødoverløb Damhusåens renseanlæg]:[Roskildevej]])","v":19800},{"$nulls":42},"Strategi",5000,5000,700,3000,1200,500,100,300,300,500,500,200,1500,0,1000,19800]
["Overløbshyppighed antal/år","Status",2,1,0.5,0.1,0.1,0.1,0.1,0.1,0.25,0.3,0.1,0.1,0.2,0,13,{"$f":"SUM(Tabel15[[#This Row],[Nødoverløb Damhusåens renseanlæg]:[Roskildevej]])","v":17.95},{"$nulls":41},"Overløbshyppighed antal/år","Status",2,1,0.5,0.1,0.1,0.1,0.1,0.1,0.25,0.3,0.1,0.1,0.2,0,13,"-"]
[null,"Plan",2,1,0.5,0.1,0.1,0.1,0.1,0.1,0.25,0.3,0.1,0.1,0.2,0,13,{"$f":"SUM(Tabel15[[#This Row],[Nødoverløb Damhusåens renseanlæg]:[Roskildevej]])","v":17.95},{"$nulls":42},"Plan",2,1,0.5,0.1,0.1,0.1,0.1,0.1,0.25,0.3,0.1,0.1,0.2,0,13,"-"]
[null,"Strategi",1,0.1,0.05,0.01,0.01,0.01,0.01,0.01,2.5000000000000001E-2,0.03,0.01,0.01,0.02,0,10,{"$f":"SUM(Tabel15[[#This Row],[Nødoverløb Damhusåens renseanlæg]:[Roskildevej]])","v":11.295},{"$nulls":42},"Strategi",1,0.1,0.05,0.01,0.01,0.01,0.01,0.01,2.5000000000000001E-2,0.03,0.01,0.01,0.02,0,10,"-"]
["Vand                         m3/år","Status",3408,15000,500,1000,100,100,100,100,500,100,100,100,500,0,8734,{"$f":"SUM(Tabel15[[#This Row],[Nødoverløb Damhusåens renseanlæg]:[Roskildevej]])","v":30342},{"$nulls":41},"Vand                         m3/år","Status",3408,15000,500,1000,100,100,100,100,500,100,100,100,500,0,8734,{"$f":"SUM(BJ17:BX17)","v":30342}]
[null,"Plan",3408,15000,500,1000,100,100,100,100,500,100,100,100,500,0,8734,{"$f":"SUM(Tabel15[[#This Row],[Nødoverløb Damhusåens renseanlæg]:[Roskildevej]])","v":30342},{"$nulls":42},"Plan",3408,15000,500,1000,100,100,100,100,500,100,100,100,500,0,8734,30342]
[null,"Strategi",1704,1500,50,100,10,10,10,10,50,10,10,10,50,0,780,{"$f":"SUM(Tabel15[[#This Row],[Nødoverløb Damhusåens renseanlæg]:[Roskildevej]])","v":4304},{"$nulls":42},"Strategi",1704,1500,50,100,10,10,10,10,50,10,10,10,50,0,780,4304]
["COD                            kg/år","Status",170.4,750,25,50,5,5,5,5,25,5,5,5,25,0,436.70000000000005,{"$f":"SUM(Tabel15[[#This Row],[Nødoverløb Damhusåens renseanlæg]:[Roskildevej]])","v":1517.1000000000001},{"$nulls":41},"COD                            kg/år","Status",170,750,25,50,5,5,5,5,25,5,5,5,25,0,437,1517]
[null,"Plan",170.4,750,25,50,5,5,5,5,25,5,5,5,25,0,436.70000000000005,{"$f":"SUM(Tabel15[[#This Row],[Nødoverløb Damhusåens renseanlæg]:[Roskildevej]])","v":1517.1000000000001},{"$nulls":42},"Plan",170,750,25,50,5,5,5,5,25,5,5,5,25,0,437,1517]
[null,"Strategi",85.2,75,2,5.9375,0.5,0.5,0.5,0.5,2.5,0.5,0.5,0.5,2.5,0,39,{"$f":"SUM(Tabel15[[#This Row],[Nødoverløb Damhusåens renseanlæg]:[Roskildevej]])","v":215.63749999999999},{"$nulls":42},"Strategi",85,75,2,5.9,0.5,0.5,0.5,0.5,2.5,0.5,0.5,0.5,2.5,0,39,215.4]
["Total N                    kg/år","Status",6.8159999999999998,30,1,2,0.2,0.2,0.2,0.2,1,0.2,0.2,0.2,1,0,17.468,{"$f":"SUM(Tabel15[[#This Row],[Nødoverløb Damhusåens renseanlæg]:[Roskildevej]])","v":60.684000000000026},{"$nulls":41},"Total N                    kg/år","Status",6.8,30,1,2,0.2,0.2,0.2,0.2,1,0.2,0.2,0.2,1,0,17.5,60.700000000000017]
[null,"Plan",6.8159999999999998,30,1,2,0.2,0.2,0.2,0.2,1,0.2,0.2,0.2,1,0,17.468,{"$f":"SUM(Tabel15[[#This Row],[Nødoverløb Damhusåens renseanlæg]:[Roskildevej]])","v":60.684000000000026},{"$nulls":42},"Plan",6.8,30,1,2,0.2,0.2,0.2,0.2,1,0.2,0.2,0.2,1,0,17.5,60.700000000000017]
[null,"Strategi",3.4079999999999999,3,0.08,0.23750000000000002,0.02,0.02,0.02,0.02,0.1,0.02,0.02,0.02,0.1,0,1.56,{"$f":"SUM(Tabel15[[#This Row],[Nødoverløb Damhusåens renseanlæg]:[Roskildevej]])","v":8.6254999999999953},{"$nulls":42},"Strategi",3.4,3,0.08,0.2,0.02,0.02,0.02,0.02,0.1,0.02,0.02,0.02,0.1,0,1.6,8.6199999999999974]
["Total P                                         kg/år","Status",1.704,7.5,0.25,0.5,0.05,0.05,0.05,0.05,0.25,0.05,0.05,0.05,0.25,0,4.367,{"$f":"SUM(Tabel15[[#This Row],[Nødoverløb Damhusåens renseanlæg]:[Roskildevej]])","v":15.171000000000006},{"$nulls":41},"Total P                                         kg/år","Status",1.7,7.5,0.25,0.5,0.05,0.05,0.05,0.05,0.25,0.05,0.05,0.05,0.25,0,4.4000000000000004,15.200000000000005]
[null,"Plan",1.704,7.5,0.25,0.5,0.05,0.05,0.05,0.05,0.25,0.05,0.05,0.05,0.25,0,4.367,{"$f":"SUM(Tabel15[[#This Row],[Nødoverløb Damhusåens renseanlæg]:[Roskildevej]])","v":15.171000000000006},{"$nulls":42},"Plan",1.7,7.5,0.25,0.5,0.05,0.05,0.05,0.05,0.25,0.05,0.05,0.05,0.25,0,4.4000000000000004,15.200000000000005]
[null,"Strategi",0.85199999999999998,0.75,0.02,5.9375000000000004E-2,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,2.5000000000000001E-2,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,2.5000000000000001E-2,0,0.39,{"$f":"SUM(Tabel15[[#This Row],[Nødoverløb Damhusåens renseanlæg]:[Roskildevej]])","v":2.1563749999999988},{"$nulls":42},"Strategi",0.8,0.75,0.02,0.06,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,2.5000000000000001E-2,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,2.5000000000000001E-2,0,0.4,{"$f":"SUM(BJ28:BX28)","v":2.1149999999999993}]