{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Kalveboderne"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Kalveboderne","index":0,"n_rows":28,"n_cols":68,"rows_kept":28,"cut":false,"hidden":false,"merged":[[19,0,21,0],[19,50,21,50],[22,0,24,0],[22,50,24,50],[25,0,27,0],[25,50,27,50],[10,0,12,0],[10,50,12,50],[13,0,15,0],[13,50,15,50],[16,0,18,0],[16,50,18,50],[3,0,3,1],[3,50,3,51],[4,0,6,0],[4,50,6,50],[7,0,9,0],[7,50,9,50],[0,0,1,1],[0,2,1,4],[0,50,1,51],[0,52,1,54],[2,0,2,1],[2,50,2,51]]}
["Vandområde",null,"Kalveboderne",{"$nulls":47},"Vandområde",null,"Damhusåen"]
[]
["Udlednings nr. ",null,"UK11","UK12","UK15","UØX4",{"$nulls":44},"Udlednings nr. ",null,"UD10b","UD10d","UD11b","UD12","UD13","UD14","UD15","UD16","UD17","UD18","UD19b","UD20b","UD21","UD21b","UD24","Sum"]
["Adresse",null,"Gåsebæk-renden","Enghave Kanal","Molestien","KV til Kalveboderne 2028","SUM",{"$nulls":43},"Adresse",null,"Nødoverløb Damhusåens renseanlæg","Hovedoverløb Damhus-ledning","Åhaven","Sønderkær","Vigerslev Allé","Gårdstedet","Heldbovej","Lykkebovej","Landlystvej","Skyttegårdsvej","Sandhusvej","Hvidovre station","Vigerslev-parken N for Dæmningen","Nødoverløb ved Torpedo-bygværket","Roskildevej","-"]
["Kloakeringstype","Status","Fælles","Fælles","Separat","-","-",{"$nulls":43},"Kloakeringstype","Status","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","-"]
[null,"Plan","Fælles","Fælles","Separat","Separat","-",{"$nulls":44},"Plan","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","-"]
[null,"Strategi","Fælles","Fælles","Separat","Separat","-",{"$nulls":44},"Strategi","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","-"]
["Reduceret areal       ha","Status",313.290322,61.807141999999999,4.4758515624999999,"-",{"$f":"SUM(Tabel112[[#This Row],[Gåsebæk-renden]:[KV til Kalveboderne 2028]])","v":379.5733155625},{"$nulls":43},"Reduceret areal       ha","Status",62.096269999999997,0,4.9262990000000002,13.292068,9.0631889999999995,1.4540759999999999,1.5233950000000001,3.503314,1.9389799999999999,4.8509120000000001,2.2999999999999998,1.07056,284.5,0,0,{"$f":"SUM(BA8:BO8)","v":390.51906299999996}]
[null,"Plan",313.290322,61.807141999999999,4.4758515624999999,4.5124999999999993,{"$f":"SUM(Tabel112[[#This Row],[Gåsebæk-renden]:[KV til Kalveboderne 2028]])","v":384.08581556249999},{"$nulls":44},"Plan",62.096269999999997,0,4.9262990000000002,13.292068,9.0631889999999995,1.4540759999999999,1.5233950000000001,3.503314,1.9389799999999999,4.8509120000000001,2.2999999999999998,1.07056,284.5,0,0,390.51906299999996]
[null,"Strategi",313.290322,61.807141999999999,4.4758515624999999,90.249999999999986,{"$f":"SUM(Tabel112[[#This Row],[Gåsebæk-renden]:[KV til Kalveboderne 2028]])","v":469.8233155625},{"$nulls":44},"Strategi",62.096269999999997,0,4.9262990000000002,13.292068,9.0631889999999995,1.4540759999999999,1.5233950000000001,3.503314,1.9389799999999999,4.8509120000000001,2.2999999999999998,1.07056,284.5,0,0,390.51906299999996]
["Maks udledning        l/s","Status",12000,3000,270,"-",{"$f":"SUM(Tabel112[[#This Row],[Gåsebæk-renden]:[KV til Kalveboderne 2028]])","v":15270},{"$nulls":43},"Maks udledning        l/s","Status",5000,5000,700,3000,1200,500,100,300,300,500,500,200,1500,0,1000,19800]
[null,"Plan",12000,3000,270,270,{"$f":"SUM(Tabel112[[#This Row],[Gåsebæk-renden]:[KV til Kalveboderne 2028]])","v":15540},{"$nulls":44},"Plan",5000,5000,700,3000,1200,500,100,300,300,500,500,200,1500,0,1000,19800]
[null,"Strategi",12000,3000,270,5420,{"$f":"SUM(Tabel112[[#This Row],[Gåsebæk-renden]:[KV til Kalveboderne 2028]])","v":20690},{"$nulls":44},"Strategi",5000,5000,700,3000,1200,500,100,300,300,500,500,200,1500,0,1000,19800]
["Overløbshyppighed antal/år","Status",6,1," ","-",{"$f":"SUM(Tabel112[[#This Row],[Gåsebæk-renden]:[KV til Kalveboderne 2028]])","v":7},{"$nulls":43},"Overløbshyppighed antal/år","Status",2,1,0.5,0.1,0.1,0.1,0.1,0.1,0.25,0.3,0.1,0.1,0.2,0,13,"-"]
[null,"Plan",1,1,0,0,{"$f":"SUM(Tabel112[[#This Row],[Gåsebæk-renden]:[KV til Kalveboderne 2028]])","v":2},{"$nulls":44},"Plan",2,1,0.5,0.1,0.1,0.1,0.1,0.1,0.25,0.3,0.1,0.1,0.2,0,13,"-"]
[null,"Strategi",0.33333333333333331,0.5,"",0,{"$f":"SUM(Tabel112[[#This Row],[Gåsebæk-renden]:[KV til Kalveboderne 2028]])","v":0.83333333333333326},{"$nulls":44},"Strategi",1,0.1,0.05,0.01,0.01,0.01,0.01,0.01,2.5000000000000001E-2,0.03,0.01,0.01,0.02,0,10,"-"]
["Vand                         m3/år","Status",80745,2646,15491.09664163961,"-",{"$f":"SUM(Tabel112[[#This Row],[Gåsebæk-renden]:[KV til Kalveboderne 2028]])","v":98882.096641639611},{"$nulls":43},"Vand                         m3/år","Status",3408,15000,500,1000,100,100,100,100,500,100,100,100,500,0,8734,{"$f":"SUM(BA17:BO17)","v":30342}]
[null,"Plan",12834.858333333332,2513.6999999999998,15491.09664163961,25000,{"$f":"SUM(Tabel112[[#This Row],[Gåsebæk-renden]:[KV til Kalveboderne 2028]])","v":55839.654974972938},{"$nulls":44},"Plan",3408,15000,500,1000,100,100,100,100,500,100,100,100,500,0,8734,30342]
[null,"Strategi",1255.8333333333333,1323,16265.651473721591,320000,{"$f":"SUM(Tabel112[[#This Row],[Gåsebæk-renden]:[KV til Kalveboderne 2028]])","v":338844.48480705492},{"$nulls":44},"Strategi",1704,1500,50,100,10,10,10,10,50,10,10,10,50,0,780,4304]
["COD                            kg/år","Status",4037.25,132.30000000000001,2478.5754626623375,"-",{"$f":"SUM(Tabel112[[#This Row],[Gåsebæk-renden]:[KV til Kalveboderne 2028]])","v":6648.1254626623377},{"$nulls":43},"COD                            kg/år","Status",170,750,25,50,5,5,5,5,25,5,5,5,25,0,437,1517]
[null,"Plan",641.74291666666659,125.685,2478.5754626623375,4000,{"$f":"SUM(Tabel112[[#This Row],[Gåsebæk-renden]:[KV til Kalveboderne 2028]])","v":7246.003379329004},{"$nulls":44},"Plan",170,750,25,50,5,5,5,5,25,5,5,5,25,0,437,1517]
[null,"Strategi",62.791666666666664,211.68,2602.5042357954549,51200,{"$f":"SUM(Tabel112[[#This Row],[Gåsebæk-renden]:[KV til Kalveboderne 2028]])","v":54076.975902462123},{"$nulls":44},"Strategi",85,75,2,5.9,0.5,0.5,0.5,0.5,2.5,0.5,0.5,0.5,2.5,0,39,215.4]
["Total N                    kg/år","Status",161.49,5.2919999999999998,154.91096641639609,"-",{"$f":"SUM(Tabel112[[#This Row],[Gåsebæk-renden]:[KV til Kalveboderne 2028]])","v":321.69296641639608},{"$nulls":43},"Total N                    kg/år","Status",6.8,30,1,2,0.2,0.2,0.2,0.2,1,0.2,0.2,0.2,1,0,17.5,60.700000000000017]
[null,"Plan",25.669716666666663,5.0274000000000001,154.91096641639609,250,{"$f":"SUM(Tabel112[[#This Row],[Gåsebæk-renden]:[KV til Kalveboderne 2028]])","v":435.60808308306275},{"$nulls":44},"Plan",6.8,30,1,2,0.2,0.2,0.2,0.2,1,0.2,0.2,0.2,1,0,17.5,60.700000000000017]
[null,"Strategi",2.5116666666666667,13.23,162.65651473721593,3200,{"$f":"SUM(Tabel112[[#This Row],[Gåsebæk-renden]:[KV til Kalveboderne 2028]])","v":3378.3981814038825},{"$nulls":44},"Strategi",3.4,3,0.08,0.2,0.02,0.02,0.02,0.02,0.1,0.02,0.02,0.02,0.1,0,1.6,8.6199999999999974]
["Total P                                         kg/år","Status",40.372500000000002,1.323,38.727741604099023,"-",{"$f":"SUM(Tabel112[[#This Row],[Gåsebæk-renden]:[KV til Kalveboderne 2028]])","v":80.423241604099019},{"$nulls":43},"Total P                                         kg/år","Status",1.7,7.5,0.25,0.5,0.05,0.05,0.05,0.05,0.25,0.05,0.05,0.05,0.25,0,4.4000000000000004,15.200000000000005]
[null,"Plan",6.4174291666666656,1.25685,38.727741604099023,62.5,{"$f":"SUM(Tabel112[[#This Row],[Gåsebæk-renden]:[KV til Kalveboderne 2028]])","v":108.90202077076569},{"$nulls":44},"Plan",1.7,7.5,0.25,0.5,0.05,0.05,0.05,0.05,0.25,0.05,0.05,0.05,0.25,0,4.4000000000000004,15.200000000000005]
[null,"Strategi",0.62791666666666668,3.3075000000000001,40.664128684303982,800,{"$f":"SUM(Tabel112[[#This Row],[Gåsebæk-renden]:[KV til Kalveboderne 2028]])","v":844.59954535097063},{"$nulls":44},"Strategi",0.8,0.75,0.02,0.06,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,2.5000000000000001E-2,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,2.5000000000000001E-2,0,0.4,{"$f":"SUM(BA28:BO28)","v":2.1149999999999993}]