{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Øresund"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Øresund","index":0,"n_rows":28,"n_cols":70,"rows_kept":28,"cut":false,"hidden":false,"merged":[[19,0,21,0],[19,52,21,52],[22,0,24,0],[22,52,24,52],[25,0,27,0],[25,52,27,52],[10,0,12,0],[10,52,12,52],[13,0,15,0],[13,52,15,52],[16,0,18,0],[16,52,18,52],[3,0,3,1],[3,52,3,53],[4,0,6,0],[4,52,6,52],[7,0,9,0],[7,52,9,52],[0,0,1,1],[0,2,1,4],[0,52,1,53],[0,54,1,56],[2,0,2,1],[2,52,2,53]]}
["Vandområde",null,"Øresund",{"$nulls":49},"Vandområde",null,"Damhusåen"]
[]
["Udlednings nr. ",null,"U4","UØX2","UØ14.1","UØ15","UØ17","UØ12.1",{"$nulls":44},"Udlednings nr. ",null,"UD10b","UD10d","UD11b","UD12","UD13","UD14","UD15","UD16","UD17","UD18","UD19b","UD20b","UD21","UD21b","UD24","Sum"]
["Adresse",null,"Pumpestation Strandvænget","AM til Øresund_20XX","Renseanlæg Damhusåen","Bypass Renseanlæg Damhusåen","Renseanlæg Lynetten","Bypass Renseanlæg Lynetten","SUM",{"$nulls":43},"Adresse",null,"Nødoverløb Damhusåens renseanlæg","Hovedoverløb Damhus-ledning","Åhaven","Sønderkær","Vigerslev Allé","Gårdstedet","Heldbovej","Lykkebovej","Landlystvej","Skyttegårdsvej","Sandhusvej","Hvidovre station","Vigerslev-parken N for Dæmningen","Nødoverløb ved Torpedo-bygværket","Roskildevej","-"]
["Kloakeringstype","Status","Fælles","-","-","-","-","-","-",{"$nulls":43},"Kloakeringstype","Status","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","-"]
[null,"Plan","Fælles","-","-","-","-","-","-",{"$nulls":44},"Plan","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","-"]
[null,"Strategi","Fælles","Separat","-","-","-","-","-",{"$nulls":44},"Strategi","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","-"]
["Reduceret areal       ha","Status",0,"-","-","-","-","-",{"$f":"SUM(Tabel117[[#This Row],[Pumpestation Strandvænget]:[Bypass Renseanlæg Lynetten]])","v":0},{"$nulls":43},"Reduceret areal       ha","Status",62.096269999999997,0,4.9262990000000002,13.292068,9.0631889999999995,1.4540759999999999,1.5233950000000001,3.503314,1.9389799999999999,4.8509120000000001,2.2999999999999998,1.07056,284.5,0,0,{"$f":"SUM(BC8:BQ8)","v":390.51906299999996}]
[null,"Plan",0,"-","-","-","-","-",{"$f":"SUM(Tabel117[[#This Row],[Pumpestation Strandvænget]:[Bypass Renseanlæg Lynetten]])","v":0},{"$nulls":44},"Plan",62.096269999999997,0,4.9262990000000002,13.292068,9.0631889999999995,1.4540759999999999,1.5233950000000001,3.503314,1.9389799999999999,4.8509120000000001,2.2999999999999998,1.07056,284.5,0,0,390.51906299999996]
[null,"Strategi",0,141.33333333333334,"-","-","-","-",{"$f":"SUM(Tabel117[[#This Row],[Pumpestation Strandvænget]:[Bypass Renseanlæg Lynetten]])","v":141.33333333333334},{"$nulls":44},"Strategi",62.096269999999997,0,4.9262990000000002,13.292068,9.0631889999999995,1.4540759999999999,1.5233950000000001,3.503314,1.9389799999999999,4.8509120000000001,2.2999999999999998,1.07056,284.5,0,0,390.51906299999996]
["Maks udledning        l/s","Status",1500,"-","-","-","-","-",{"$f":"SUM(Tabel117[[#This Row],[Pumpestation Strandvænget]:[Bypass Renseanlæg Lynetten]])","v":1500},{"$nulls":43},"Maks udledning        l/s","Status",5000,5000,700,3000,1200,500,100,300,300,500,500,200,1500,0,1000,19800]
[null,"Plan",1500,"-","-","-","-","-",{"$f":"SUM(Tabel117[[#This Row],[Pumpestation Strandvænget]:[Bypass Renseanlæg Lynetten]])","v":1500},{"$nulls":44},"Plan",5000,5000,700,3000,1200,500,100,300,300,500,500,200,1500,0,1000,19800]
[null,"Strategi",1500,8480,"-","-","-","-",{"$f":"SUM(Tabel117[[#This Row],[Pumpestation Strandvænget]:[Bypass Renseanlæg Lynetten]])","v":9980},{"$nulls":44},"Strategi",5000,5000,700,3000,1200,500,100,300,300,500,500,200,1500,0,1000,19800]
["Overløbshyppighed antal/år","Status",15,"-","-","-","-","-",{"$f":"SUM(Tabel117[[#This Row],[Pumpestation Strandvænget]:[Bypass Renseanlæg Lynetten]])","v":15},{"$nulls":43},"Overløbshyppighed antal/år","Status",2,1,0.5,0.1,0.1,0.1,0.1,0.1,0.25,0.3,0.1,0.1,0.2,0,13,"-"]
[null,"Plan",15,"-","-","-","-","-",{"$f":"SUM(Tabel117[[#This Row],[Pumpestation Strandvænget]:[Bypass Renseanlæg Lynetten]])","v":15},{"$nulls":44},"Plan",2,1,0.5,0.1,0.1,0.1,0.1,0.1,0.25,0.3,0.1,0.1,0.2,0,13,"-"]
[null,"Strategi",15,0,"-","-","-","-",{"$f":"SUM(Tabel117[[#This Row],[Pumpestation Strandvænget]:[Bypass Renseanlæg Lynetten]])","v":15},{"$nulls":44},"Strategi",1,0.1,0.05,0.01,0.01,0.01,0.01,0.01,2.5000000000000001E-2,0.03,0.01,0.01,0.02,0,10,"-"]
["Vand                         m3/år","Status",105000,"-",{"$nulls":4},{"$f":"SUM(Tabel117[[#This Row],[Pumpestation Strandvænget]:[Bypass Renseanlæg Lynetten]])","v":105000},{"$nulls":43},"Vand                         m3/år","Status",3408,15000,500,1000,100,100,100,100,500,100,100,100,500,0,8734,{"$f":"SUM(BC17:BQ17)","v":30342}]
[null,"Plan",105000,"-",{"$nulls":4},{"$f":"SUM(Tabel117[[#This Row],[Pumpestation Strandvænget]:[Bypass Renseanlæg Lynetten]])","v":105000},{"$nulls":44},"Plan",3408,15000,500,1000,100,100,100,100,500,100,100,100,500,0,8734,30342]
[null,"Strategi",45453.75,500000,{"$nulls":4},{"$f":"SUM(Tabel117[[#This Row],[Pumpestation Strandvænget]:[Bypass Renseanlæg Lynetten]])","v":545453.75},{"$nulls":44},"Strategi",1704,1500,50,100,10,10,10,10,50,10,10,10,50,0,780,4304]
["COD                            kg/år","Status",5250,"-",875000,535000,2505000,1493000,{"$f":"SUM(Tabel117[[#This Row],[Pumpestation Strandvænget]:[Bypass Renseanlæg Lynetten]])","v":5413250},{"$nulls":43},"COD                            kg/år","Status",170,750,25,50,5,5,5,5,25,5,5,5,25,0,437,1517]
[null,"Plan",5250,"-",889000,173000,1965000,310000,{"$f":"SUM(Tabel117[[#This Row],[Pumpestation Strandvænget]:[Bypass Renseanlæg Lynetten]])","v":3342250},{"$nulls":44},"Plan",170,750,25,50,5,5,5,5,25,5,5,5,25,0,437,1517]
[null,"Strategi",2272.6875,80000,833000,135000,1832000,220000,{"$f":"SUM(Tabel117[[#This Row],[Pumpestation Strandvænget]:[Bypass Renseanlæg Lynetten]])","v":3102272.6875},{"$nulls":44},"Strategi",85,75,2,5.9,0.5,0.5,0.5,0.5,2.5,0.5,0.5,0.5,2.5,0,39,215.4]
["Total N                    kg/år","Status",210,"-",195000,67000,425000,117000,{"$f":"SUM(Tabel117[[#This Row],[Pumpestation Strandvænget]:[Bypass Renseanlæg Lynetten]])","v":804210},{"$nulls":43},"Total N                    kg/år","Status",6.8,30,1,2,0.2,0.2,0.2,0.2,1,0.2,0.2,0.2,1,0,17.5,60.700000000000017]
[null,"Plan",210,"-",163000,19000,360000,24000,{"$f":"SUM(Tabel117[[#This Row],[Pumpestation Strandvænget]:[Bypass Renseanlæg Lynetten]])","v":566210},{"$nulls":44},"Plan",6.8,30,1,2,0.2,0.2,0.2,0.2,1,0.2,0.2,0.2,1,0,17.5,60.700000000000017]
[null,"Strategi",90.907499999999999,5000,153000,15000,336000,17000,{"$f":"SUM(Tabel117[[#This Row],[Pumpestation Strandvænget]:[Bypass Renseanlæg Lynetten]])","v":526090.90749999997},{"$nulls":44},"Strategi",3.4,3,0.08,0.2,0.02,0.02,0.02,0.02,0.1,0.02,0.02,0.02,0.1,0,1.6,8.6199999999999974]
["Total P                                         kg/år","Status",52.5,"-",25000,10100,78000,20700,{"$f":"SUM(Tabel117[[#This Row],[Pumpestation Strandvænget]:[Bypass Renseanlæg Lynetten]])","v":133852.5},{"$nulls":43},"Total P                                         kg/år","Status",1.7,7.5,0.25,0.5,0.05,0.05,0.05,0.05,0.25,0.05,0.05,0.05,0.25,0,4.4000000000000004,15.200000000000005]
[null,"Plan",52.5,"-",15000,2800,33000,4200,{"$f":"SUM(Tabel117[[#This Row],[Pumpestation Strandvænget]:[Bypass Renseanlæg Lynetten]])","v":55052.5},{"$nulls":44},"Plan",1.7,7.5,0.25,0.5,0.05,0.05,0.05,0.05,0.25,0.05,0.05,0.05,0.25,0,4.4000000000000004,15.200000000000005]
[null,"Strategi",22.726875,1250,14000,2200,31000,3000,{"$f":"SUM(Tabel117[[#This Row],[Pumpestation Strandvænget]:[Bypass Renseanlæg Lynetten]])","v":51472.726875},{"$nulls":44},"Strategi",0.8,0.75,0.02,0.06,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,2.5000000000000001E-2,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,2.5000000000000001E-2,0,0.4,{"$f":"SUM(BC28:BQ28)","v":2.1149999999999993}]