{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Svanemøllebugten"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Svanemøllebugten","index":0,"n_rows":28,"n_cols":72,"rows_kept":28,"cut":false,"hidden":false,"merged":[[19,0,21,0],[19,54,21,54],[22,0,24,0],[22,54,24,54],[25,0,27,0],[25,54,27,54],[10,0,12,0],[10,54,12,54],[13,0,15,0],[13,54,15,54],[16,0,18,0],[16,54,18,54],[3,0,3,1],[3,54,3,55],[4,0,6,0],[4,54,6,54],[7,0,9,0],[7,54,9,54],[0,0,1,1],[0,2,1,4],[0,54,1,55],[0,56,1,58],[2,0,2,1],[2,54,2,55]]}
["Vandområde",null,"Svanemøllebugten",{"$nulls":51},"Vandområde",null,"Damhusåen"]
[]
["Udlednings nr. ",null,"UØ10.1","UØ10.2","UØ14.1","UØ15","UØ17","UØ12.1","UØ16","UØX3",{"$nulls":44},"Udlednings nr. ",null,"UD10b","UD10d","UD11b","UD12","UD13","UD14","UD15","UD16","UD17","UD18","UD19b","UD20b","UD21","UD21b","UD24","Sum"]
["Adresse",null,"Vilhelms-dalsløbet","Scherfigsvej N","Strandvænget","Lautrupkaj","Sundkrogs-gade","Svaneknoppen","Lautrupsgade","BIR til Svanemølle-bugten 2028","SUM",{"$nulls":43},"Adresse",null,"Nødoverløb Damhusåens renseanlæg","Hovedoverløb Damhus-ledning","Åhaven","Sønderkær","Vigerslev Allé","Gårdstedet","Heldbovej","Lykkebovej","Landlystvej","Skyttegårdsvej","Sandhusvej","Hvidovre station","Vigerslev-parken N for Dæmningen","Nødoverløb ved Torpedo-bygværket","Roskildevej","-"]
["Kloakeringstype","Status","Fælles","Fælles","Fælles","Fælles","Fælles","Separat","Separat","-","-",{"$nulls":43},"Kloakeringstype","Status","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","-"]
[null,"Plan","Fælles","Fælles","Fælles","Fælles","Fælles","Separat","Separat","Separat","-",{"$nulls":44},"Plan","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","-"]
[null,"Strategi","Fælles","Fælles","Fælles","Fælles","Fælles","Separat","Separat","Separat","-",{"$nulls":44},"Strategi","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","Fælles","-"]
["Reduceret areal       ha","Status",371.9,21.743694000000001,136.18926300000001,8.6407489999999996,32.538127000000003,2.20533125,0.92470312499999996,"-",{"$f":"SUM(C8:J8)","v":574.14186737499995},{"$nulls":43},"Reduceret areal       ha","Status",62.096269999999997,0,4.9262990000000002,13.292068,9.0631889999999995,1.4540759999999999,1.5233950000000001,3.503314,1.9389799999999999,4.8509120000000001,2.2999999999999998,1.07056,284.5,0,0,{"$f":"SUM(BE8:BS8)","v":390.51906299999996}]
[null,"Plan",371.9,21.743694000000001,136.18926300000001,8.6407489999999996,32.538127000000003,2.20533125,0.92470312499999996,7.6050000000000013,{"$f":"SUM(C9:J9)","v":581.74686737499997},{"$nulls":44},"Plan",62.096269999999997,0,4.9262990000000002,13.292068,9.0631889999999995,1.4540759999999999,1.5233950000000001,3.503314,1.9389799999999999,4.8509120000000001,2.2999999999999998,1.07056,284.5,0,0,390.51906299999996]
[null,"Strategi",371.9,21.743694000000001,136.18926300000001,8.6407489999999996,32.538127000000003,2.20533125,0.92470312499999996,152.1,726.24186737499997,{"$nulls":44},"Strategi",62.096269999999997,0,4.9262990000000002,13.292068,9.0631889999999995,1.4540759999999999,1.5233950000000001,3.503314,1.9389799999999999,4.8509120000000001,2.2999999999999998,1.07056,284.5,0,0,390.51906299999996]
["Maks udledning        l/s","Status",16000,500,5000,100,2000,130,60,"-",23790,{"$nulls":43},"Maks udledning        l/s","Status",5000,5000,700,3000,1200,500,100,300,300,500,500,200,1500,0,1000,19800]
[null,"Plan",16000,500,5000,100,2000,130,60,460,24250,{"$nulls":44},"Plan",5000,5000,700,3000,1200,500,100,300,300,500,500,200,1500,0,1000,19800]
[null,"Strategi",16000,500,5000,100,2000,130,60,9130,32920,{"$nulls":44},"Strategi",5000,5000,700,3000,1200,500,100,300,300,500,500,200,1500,0,1000,19800]
["Overløbshyppighed antal/år","Status",12,1,9,1,2," "," ","-",25,{"$nulls":43},"Overløbshyppighed antal/år","Status",2,1,0.5,0.1,0.1,0.1,0.1,0.1,0.25,0.3,0.1,0.1,0.2,0,13,"-"]
[null,"Plan",12,1,9,1,2,0,0,0,25,{"$nulls":44},"Plan",2,1,0.5,0.1,0.1,0.1,0.1,0.1,0.25,0.3,0.1,0.1,0.2,0,13,"-"]
[null,"Strategi",2,1,4,1,1,"","",0,9,{"$nulls":44},"Strategi",1,0.1,0.05,0.01,0.01,0.01,0.01,0.01,2.5000000000000001E-2,0.03,0.01,0.01,0.02,0,10,"-"]
["Vand                         m3/år","Status",345728,11730,50433,24,2209,7843.4894457547161,3288.8026238207544,"-",421256.29206957552,{"$nulls":43},"Vand                         m3/år","Status",3408,15000,500,1000,100,100,100,100,500,100,100,100,500,0,8734,{"$f":"SUM(BE17:BS17)","v":30342}]
[null,"Plan",330577.5,11279.95,48425.9,22.95,2113.6999999999998,7843.4894457547161,3288.8026238207544,42000,445552.29206957557,{"$nulls":44},"Plan",3408,15000,500,1000,100,100,100,100,500,100,100,100,500,0,8734,30342]
[null,"Strategi",53397.5,3411.25,12863.75,3.75,378.75,8235.6639180424518,3453.2427550117923,540000,621743.90667305421,{"$nulls":44},"Strategi",1704,1500,50,100,10,10,10,10,50,10,10,10,50,0,780,4304]
["COD                            kg/år","Status",17286.400000000001,586.5,2521.65,1.2000000000000002,110.45,1254.9583113207545,526.20841981132071,"-",22287.366731132082,{"$nulls":43},"COD                            kg/år","Status",170,750,25,50,5,5,5,5,25,5,5,5,25,0,437,1517]
[null,"Plan",16528.875,563.99750000000006,2421.2950000000001,1.1475,105.685,1254.9583113207545,526.20841981132071,6720,28122.166731132078,{"$nulls":44},"Plan",170,750,25,50,5,5,5,5,25,5,5,5,25,0,437,1517]
[null,"Strategi",2669.875,170.5625,643.1875,0.1875,18.9375,1317.7062268867924,552.51884080188677,86400,91772.975067688676,{"$nulls":44},"Strategi",85,75,2,5.9,0.5,0.5,0.5,0.5,2.5,0.5,0.5,0.5,2.5,0,39,215.4]
["Total N                    kg/år","Status",691.45600000000002,23.46,100.866,4.8000000000000001E-2,4.4180000000000001,78.434894457547159,32.888026238207544,"-",931.57092069575481,{"$nulls":43},"Total N                    kg/år","Status",6.8,30,1,2,0.2,0.2,0.2,0.2,1,0.2,0.2,0.2,1,0,17.5,60.700000000000017]
[null,"Plan",661.15499999999997,22.559900000000003,96.851800000000011,4.5899999999999996E-2,4.2273999999999994,78.434894457547159,32.888026238207544,420,1316.1629206957546,{"$nulls":44},"Plan",6.8,30,1,2,0.2,0.2,0.2,0.2,1,0.2,0.2,0.2,1,0,17.5,60.700000000000017]
[null,"Strategi",106.795,6.8224999999999998,25.727499999999999,7.4999999999999997E-3,0.75750000000000006,82.356639180424523,34.532427550117923,5400,5656.9990667305428,{"$nulls":44},"Strategi",3.4,3,0.08,0.2,0.02,0.02,0.02,0.02,0.1,0.02,0.02,0.02,0.1,0,1.6,8.6199999999999974]
["Total P                                         kg/år","Status",172.864,5.8650000000000002,25.2165,1.2E-2,1.1045,19.60872361438679,8.2220065595518861,"-",232.8927301739387,{"$nulls":43},"Total P                                         kg/år","Status",1.7,7.5,0.25,0.5,0.05,0.05,0.05,0.05,0.25,0.05,0.05,0.05,0.25,0,4.4000000000000004,15.200000000000005]
[null,"Plan",165.28874999999999,5.6399750000000006,24.212950000000003,1.1474999999999999E-2,1.0568499999999998,19.60872361438679,8.2220065595518861,105,329.04073017393864,{"$nulls":44},"Plan",1.7,7.5,0.25,0.5,0.05,0.05,0.05,0.05,0.25,0.05,0.05,0.05,0.25,0,4.4000000000000004,15.200000000000005]
[null,"Strategi",26.69875,1.7056249999999999,6.4318749999999998,1.8749999999999999E-3,0.18937500000000002,20.589159795106131,8.6331068875294807,1350,1414.2497666826357,{"$nulls":44},"Strategi",0.8,0.75,0.02,0.06,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,2.5000000000000001E-2,5.0000000000000001E-3,5.0000000000000001E-3,5.0000000000000001E-3,2.5000000000000001E-2,0,0.4,{"$f":"SUM(BE28:BS28)","v":2.1149999999999993}]